Hotel Alarm Clock Outage Test Checklist
Proposed sample acceptance procedure. Example timings are not certification requirements. Use one record per unit and configuration. Not tested means unresolved. Agree exclusions in writing before approval.
Property / tester / date: __________________________________________________________
Unit ID / model / revision / adapter: ______________________________________________
Battery type / installation date / alarm mode / volume: ______________________________
Required outage duration / timing tolerance / reference clock: ________________________
	Check
	Required observation or record
	Acceptance basis
	Observed result / status
	Corrective action / owner

	Identity and baseline
	Record unit, model/revision, adapter, battery, settings, tester, and date. Confirm normal-powered alarm.
	Matches the proposed supplied configuration; baseline works.
	
	

	Battery readiness
	Check specified cell, correct installation, activation tab, door closure, and any warning.
	Installed as instructed; no unresolved low-battery warning.
	
	

	Short interruption
	Set alarm five minutes ahead; disconnect one minute later; remain unplugged past due time.
	Audible alarm meets the agreed timing and sound requirement.
	
	

	Display and controls
	Observe display; test stop and snooze during the battery-powered alarm.
	Behavior documented and matches required guest functions.
	
	

	Sound fallback
	Repeat each intended alarm mode with unavailable external audio where relevant.
	Approved fallback or limitation is confirmed.
	
	




Hotel Alarm Clock Outage Test Checklist
Proposed sample acceptance procedure. Example timings are not certification requirements. Use one record per unit and configuration. Not tested means unresolved. Agree exclusions in writing before approval.
Unit ID / tester / date: __________________________________________________________
	Check
	Required observation or record
	Acceptance basis
	Observed result / status
	Corrective action / owner

	Required duration
	Run a separate trial for the agreed outage duration; alarm due near its end.
	Alarm sounds while power is absent; actual duration recorded.
	
	

	Charging
	Check USB and wireless charging during the interruption, where fitted.
	Actual behavior recorded; meets any separately specified requirement.
	
	

	Power restoration
	Use separate trials restoring power before, during, and after the due alarm.
	Time, armed state, sound, and restart behavior match agreed criteria.
	
	

	Battery service and reset
	Follow the approved battery replacement procedure; restore settings and repeat the alarm test.
	Service completed, door secured, settings checked, and retest passed.
	
	

	Room release
	Verify local time, intended alarm state, room placement, and completed actions.
	No required test unresolved; responsible approver signs the record.
	
	


Status for every row: Pass / Fail / Not tested. Record actual duration and alarm time in the observations.
Release decision / approver / date: __________________________________________________
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